15A NCAC 05C .0115 REMOVAL

All pipe used in geophysical operations shall be removed by the permittee using such pipe to at least six feet below the bottom of the water body and in charted navigable channels, eight feet below charted dredge depth before leaving the location where the pipe is placed.

History Note: Authority G.S. 113‑391;

Eff. February 1, 1976;

Readopted Eff. August 1, 1982;

Readopted Eff. July 1, 2025.