15A NCAC 05C .0119 SHOOTING

(a) No shot shall be allowed except in daylight hours. Shot is defined in 15A NCAC 05C .0101(i).

(b) No shot shall be allowed in heavy fog.

(c) The permittee shall stop gas and water spouts caused by drilling or shooting operations of seismic crews as soon as possible, but no later than 24 hours after the spout is first noticed.

History Note: Authority G.S. 113‑391;

Eff. February 1, 1976;

Readopted Eff. August 1, 1982;

Readopted Eff. July 1, 2025.