15A NCAC 05C .0117 PIPES AND BUOYS

All pipes, buoys, and other markers used in connection with seismic work shall be flagged in the daytime and lighted at night according to the navigation rules of the U.S. Army Corps of Engineers and the U.S. Coast Guard.

History Note: Authority G.S. 113‑391;

Eff. February 1, 1976;

Readopted Eff. August 1, 1982;

Readopted Eff. July 1, 2025.