**NC Division of Energy, Mineral, and Land Resources**

**Operation & Maintenance Inspection Form – Stormwater Wetland**

|  |  |  |
| --- | --- | --- |
| Project name: | Permit number:  SW | Inspection date: |
| Street address: | City: | State and ZIP code: |
| Name of inspector: | Phone number: | Email address: |
| Description of SCM location on the project: | | |
| Signature of Inspector certifying that the information provided in this form is complete and correct: | | |

|  |  |
| --- | --- |
| **Stormwater Collection System and Accessibility** | |
| 1. Swales are free from blockage and erosion. | Yes  No  N/A |
| 1. Grates, gutters, curb openings, and pipes appear free from damage and clogs. | Yes  No  N/A |
| 1. The stormwater wetland is accessible for inspection. | Yes  No  N/A |
| **Inlet(s) and Forebay** | |
| 1. Inlet(s) are free from damage, clogs, and erosion. | Yes  No  N/A |
| 1. Forebay berm is stable and not eroding. | Yes  No  N/A |
| 1. Cattails, phragmites or other invasive plants cover < 10% of the surface area. | Yes  No  N/A |
| 1. Forebay is free from trash and debris. | Yes  No  N/A |
| 1. Forebay is at least 15 inches deep. | Yes  No  N/A |
| **Perimeter, Embankment, and Side Slopes** | |
| 1. Perimeter is free from water quality impacts caused by geese and ducks. | Yes  No  N/A |
| 1. Embankment is free from woody shrubs and trees. | Yes  No  N/A |
| 1. Side slopes are stable, vegetated, and free from erosion/bare soil. | Yes  No  N/A |
| 1. Side slopes are free from trash and debris. | Yes  No  N/A |
| 1. Side slopes are free from muskrat and/or beaver activity. | Yes  No  N/A |
| **Shallow Water and Temporary Inundation Zone(s)** | |
| 1. Shallow water/temporary inundation zones are covered with healthy vegetation. | Yes  No  N/A |
| 1. Shallow water and temporary inundation zones are free from erosion. | Yes  No  N/A |
| 1. Cattails, phragmites or other invasive plants cover < 10% of the surface area. | Yes  No  N/A |
| 1. Temporary inundation zones are drained within 5 days after a storm event. | Yes  No  N/A |
| 1. Shallow water and temporary inundation zones are free from trash and debris. | Yes  No  N/A |
| **Deep Pools** | |
| 1. Deep pools are at least 15 inches deep. | Yes  No  N/A |
| 1. Cattails, phragmites, or other invasive plants cover < 10% of the surface area. | Yes  No  N/A |
| 1. Deep pools are free from trash and debris. | Yes  No  N/A |
| 1. Standing water is present in deep pools. | Yes  No  N/A |
| 1. Deep pool adjacent to the outlet structure is free of vegetation. | Yes  No  N/A |

|  |  |  |  |
| --- | --- | --- | --- |
| **Outlet Device(s)** | | | |
| 1. Emergency bypass and/or bypass swale is clearly visible and in good condition. | | Yes  No  N/A | |
| 1. Outlet structure is free from damage, clogs, and erosion. | | Yes  No  N/A | |
| 1. Water level matches the level of the lowest outlet. | | Yes  No  N/A | |
|  | |  |
| **Action Plan to address any “Nos” listed above, including dates for completion (for permittee to complete):** | | |
|  | | |