**Meeting Objectives**

*For TAG members to have the opportunity to achieve consensus on the following:*

* Tiered BUA thresholds for post-construction stormwater requirements, including basic treatment requirements at each
* Volume reduction requirement
* Stream protection criteria
* {possible} Post-construction stormwater treatment requirement applicability trigger

|  |  |
| --- | --- |
| Agenda |  |
| 10 am | **Welcome, meeting purpose, introductions, working together** |
| 10:10 pm  *20 minutes* | **Present, discuss & consensus check on tiered thresholds**  (10 minutes)   * Discuss 6%/12% BUA cutoff * Addition of SCM requirements above 6% or when stormwater collection system is present or proposed   (10 minutes)   * Call to question * Go-around: your rationale for your vote |
| 10:30 am  *20 minutes* | **Present, discuss & consensus check on volume reduction requirement**  (10 minutes)   * Applies above 12% BUA or with stormwater collection system * Optional 90th percentile design storm size without volume reduction * Incentivizes stormwater recharge   (10 minutes)   * Call to question * Go-around: your rationale for your vote |
| 10:50 am  *20 minutes* | **Present, discuss & consensus check on stream protection criteria**  (10 minutes)   * Applies above 12% BUA * Protects against prolonged erosive flows * Exemptions where little to no benefit can be demonstrated  1. inutes)  * Call to question & Go-around: your rationale for your vote |
| 11:10 am  *30 minutes* | **Present and discuss applicability trigger**   * 1 acre disturbance threshold * Exemptions * {Possible} call to question * Exemptions |
| 11:40 am  *20 minutes* | **Next steps** |
| Noon | **Adjourn** |